**Instructions Model 377**

1. unscrew the push plate on your piggyback adapter.
2. The push plate is a small silver circular plate that comes attached to the piggyback adapter (BRP-10).
3. Unscrew the larger size push plate that is attached to your model 377 at the end of the rod.
4. Pull the rod back until you can fit the piggyback adapter inside of the 377's half barrel.
5. Push the rod through the piggyback adapter until the rod is fully extended.
6. Screw your small push plate that was originally attached to the piggyback adapter onto the end of the rod
7. Insert 10oz tube into the cradle with roll pulled all the way back.